N° : 5140289	Date : 18 janv. 2019	

Induction motor with options	
2P LSES 80LG 1,1kW IFT/IE3  B35 208VYY/230VYY/460VY 60Hz	
Connection network material Aluminium alloy ; Metal cover ; 	

Utilisation : Environment Current ; Ambiance Non corrosive ; Finition - ; Zone Non specific ; General applications ; Ambient temperature -16 +40 °C ; Maximum altitude 1000 m.		
Motor caracteristics : Aluminium alloy housing ; Cast iron DE endshield ; Aluminium alloy NDE endshield. 		

Motor definition
Protection type	-		Application	General applications	
Generation code	IFT		Main voltage (V)	460	
Efficiency class	IE3		Connection	YY/Y	
Number of network phases	3		 Motor winding (V)	208VYY/230VYY/460VY	
Number of speed			 Rated Frequency (Hz)	60	
Polarity	2P		Operation position	IM2001(IMB35)	
Motor serie	LSES		Index of protection	IP55	
Frame size (mm)	80		Index of cooling	IC411	
Lenght code	LG		Insulation class	F	
HS rated power (kW)	1.100		Finish	-	
	-		Moment of inertia J (kg.m2)	0.0022300	
Rated speed (min-1)	2885		Motor weight (kg)	14.1	
Maximum mechanical speed (min-1)	11700				

Common definitions 
Paint shade	RAL6000				
Paint system	Ia (1 polyurethane coat 20/30 microns)	

Motor mechanical interface
Mounting flange	FF165		Shaft material type	Steel shaft	
Drive end shaft type	IEC STANDARD shaft end		Nuance of shaft material	-	
Diameter DE shaft (mm)	19j6		Second shaft extension	-	
Length DE shaft (mm)	40		Diameter NDE shaft (mm)	-	
DE bearing mounting	Locked 		Second shaft end length (mm)	-	
DE bearing type	DE ball bearing		NDE bearing type	NDE ball bearing	
DE bearing	6205		NDE bearing	6204	
Code Type de graissage	Vie				

Motor electrical interface
Connection network type	Terminal box		Cable type	-	
Connection network material	Aluminium alloy		Cable gland material	Cable gland not supplied, holes tapped with polyamide plugs	
Connection network position	A		Main cable glan type	1xM20 ; With plugs	
Connection network orientation	up		Principal cable gland position	Right (1)	
Connection network relative position	0				

N° : 5140289	Date : 18 janv. 2019	

Induction motor with options - 2P LSES 80LG 1,1kW IFT/IE3  B35 208VYY/230VYY/460VY 60Hz
	Motor options
Vibration level	A (25µm ; 1.6mm/s ; 2.5m/s²)		Cover	Metal cover	
Balancing type	Half-key (H)		Drip proof cover option	-	
Impregnation type	< 95% ; -16+40°C (T)		cooling type	-	
Winding thermal protection	-		Forced ventilation caracteristics	-	
Space heater	-		Encoder type	-	
Draining plugs position	6H		Encoder caracteristics	-	
Nameplate material	Aluminium nameplate		Screw material	Steel screw	
Endshield thermal protection	-		Adaptation for vibration sensor	-	
Reinforced insulation system	-				

 
Motor characteristics (on mains supply)

Main voltage (V)	Rated Frequency (Hz)	HS rated power (kW)	Rated torque (N.m)	Rated speed (min-1)	Rated current (A)	Power factor at 4/4 of the load	Power factor at 3/4 of the load	Power factor at 2/4 of the load	Efficiency at 4/4 (IEC 60 034-2-1) of the load (%)	Efficiency at 3/4 (IEC 60 034-2-1) of the load (%)	Efficiency at 2/4 (IEC 60 034-2-1) of the load (%)	

460	60	1.100	3,65	3505.00	1.95	0.83			84.87			

Motor characteristics (on mains supply) 460 V 60 Hz
Starting torque (N.m)	9.67		Id / In	6.85	
Average starting torque (N.m)			Id	15.41	
Maximum torque (N.m)	11,86		Maximun current (A)		
Unload maximum starting frequency (d/h)	-		No-load current (A)	0.00	
Rotor locked time (cold) (s)			Acoustic pressure level (dB(A))	64	

N° : 5140289	Date : 18 janv. 2019	

Induction motor with options - 2P LSES 80LG 1,1kW IFT/IE3  B35 208VYY/230VYY/460VY 60Hz	

	

A	125	

a	45	

AA	31	

AB	157	

AC	189.00	

B	100	

BB	125	

C	70.0	

D	19j6	

E	40	

F	6	

G	15.5	

GD	6	

H	80	

HA	10	

HJ	137.0	

I	53	

II	53	

J	90	

K	9	

L	30	

LA	10	

LB	263.0	

LJ	43.5	

LO	6	

M	165	

N	130	

n	4	

O	M6	

P	200	

p	16	

rs	0.5	

S	12	

T	3.5	

ts	2	

ts1	20	

x	14